

Professional Cubicle Curtains

1-800-258-8817 • custsvc@ModoMed.com

[www.ModoMed.com](http://www.modomed.com/)

**CUBICLE CURTAIN CARE AND SPECIFICATIONS**

**FABRIC:** Chateau

**FEATURES:**

* Woven of 45% AVORA FR Blend™ polyester and 55% regular polyester yarn for inherent and permanent flame resistance.
* Permanently flame retardant passing the NFPA 701 and California Fire Marshall Title 19 vertical flammability test.

**SPECIFICATIONS:**

* Fabric Content: 45% AVORA FR Blend™ Polyester / 55% Polyester
* Finish: Fire-Retardant

**CARE INSTRUCTIONS:**

*THIS FABRIC CAN BE WASHED OR DRY CLEANED*

*WASH CYCLE:*

Machine wash in water temperature not exceeding 160oF. Using SYNTHETIC detergent.

* DO NOT BLEACH.
* DO NOT EXTRACT.
* AVOID FABRIC SOFTNERS OR OTHER CHEMICAL THAT CONTAINS SILICONE, WHICH AFFECTS FLAMMABILITY.

*DRYING CYCLE:*

* Tumble dry 3-5 minutes on SYNTHETIC cycle (110oF.) until damp dry, and remove immediately.

*FINISHING:*

* No finishing if fabric is re-hung at termination of drying cycle. Occasional light touch-up with hand iron (275oF. Maximum) may be desired.
* DO NOT MANGLE.