

Professional Cubicle Curtains

1-800-258-8817 • [custsvc@ModoMed.com](mailto:custsvc@modomed.com)

[www.ModoMed.com](http://www.modomed.com/)

**CUBICLE CURTAIN CARE AND SPECIFICATIONS**

**FABRIC:** Shoreline

**FEATURES:**

* Fabric is woven with 57% Recycled FR Polyester, 40% FR Polyester, 3% X-Static Silver Antimicrobial Fiber.
* Antimicrobial treatment prevents cross contamination and microorganisms from growing on fabric.
* This fabric can contribute to LEED Certification and contains recycled silver.
* This product has been proven effective after 200 commercial launderings.
* Permanently flame retardant passing the NFPA 701 vertical flammability test.

**SPECIFICATIONS:**

* Fabric Content: 57% Recycled FR Polyester, 40% FR Polyester, 3% X-Static Silver Antimicrobial Fiber
* Finish: Anti-Microbial Fire-Retardant
* Horizontal Repeat: 72”
* Vertical Repeat: 54”
* Lightfastness 60 hrs: 4.5
* (VOC) Volatile Organic Emission Test: Tested for Formaldehyde Emissions and Total Volatile Organic Compounds. Results: Non-detectable

**CARE INSTRUCTIONS:**

*THIS FABRIC CAN BE WASHED OR DRY CLEANED*

*WASH CYCLE:*

Machine wash in water temperature not exceeding 160oF. Using SYNTHETIC detergent.

* DO NOT USE: bleach, Sodium Hypochlorite, Sodium Hyposulfite, Sodium Silicate, Hydrogen Peroxide, and Per(oxy)Acetic Acid (PAA), Sulfer, Ammonium Sulfide, Chlorine, Strong Acids or Strong Oxidizing Agents.
* DO NOT EXTRACT.
* AVOID FABRIC SOFTNERS OR OTHER CHEMICAL THAT CONTAINS SILICONE, WHICH AFFECTS FLAMMABILITY.

*DRYING CYCLE:*

* Tumble dry 3-5 minutes on SYNTHETIC cycle (110oF.) until damp dry, and remove immediately.

*FINISHING:*

* No finishing if fabric is re-hung at termination of drying cycle.
* DO NOT MANGLE.